Change history 
for the IO-Link IODD zip file:"ThinkTop IO-Link, device descriptions (IODD)"


Rev 1 -> Rev 2
With the new functionality implemented in the ThinkTop V50 and V70’s, new IODD’s and Interface Descriptions have also been generated.
Both new and old IODD’s are included in the 2nd revision of the “ThinkTop IO-Link zip-file”.
It’s recommended to just add them all to the preferred configuration tool. The configuration tool will automatically match the correct IODD with the connected ThinkTop.


Rev 2 -> Rev 3
 The serial number parameter has been enabled in the Identification section, for the IODDs for the AE variants
  Due to formal demand from the IO-Link certification process
  It is not consideret relevant for the customer, thus the Rev2 IODDs are OK as well


Rev 3 -> Rev 4
IODD for ThinkTop V20 IO-Link added